1. **Lighting Equipment**

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Item** | **Model** | **Specification** | **Weight** | **Quantity** | **Origin** | **Remarks** |
| Dimmer | CD80sv | 5.5kW  (max 4kW) |  | 610 | Strand Lighting |  |
| Console | MA3 Light | 4096 (Parameters Mode 2) | 33kg | 2 | MA Lighting | 6 x DMX out |
| Splitter | XPD-28 | 2:8 DMX Splitter, 5-pin XLR | 1.7kg | 3 | Swisson |  |

**Light**

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Item** | **Model** | **Lamp type** | **Angle** | **Weight** | **Quantity** | **Origin** | **Remarks** |
| Follow |  | 3kW |  |  | 4 | USHIO | 2 CL Installed |
| LED Profile | Khamsin-S | White LED module | 7˚~58˚ | 40kg | 20 | Ayrton | PIT Storage |
| LED Profile | Axcor Beam300 | 110W White LED  215 VA | 2˚ | 17.6kg | 8 | Clay paky | PIT Storage |
| LED Wash | Quantum Wash | 50 X 15W LED RGBW | 11˚~53˚ | 21kg | 20 | Martin | PIT Storage |
| LED Wash | Color Force 72 Ⅱ | 12 LED engines, 24(6xRGBA)LEDs, 299 total LEDs | 23˚ | 22kg | 15 | Chroma-Q | Upper Horizont Batten- 10EA installed (고정)  PIT Storage- 5EA |
| Profile | Europe DN205 | CP79 2kW | 10˚~22˚ | 22.9kg | 59 | ADB | 1 CL-33EA  2 CL-26EA  installed |
| Fresnel | Europe F201 | CP79 2kW | 12˚~61˚ | 9.6kg | 100 | ADB | 2 Apron-4EA  1 Apron-16EA  1~5 SUS-16EA  installed |
| Fresnel |  | 5kw |  |  | 3 | Marumo | #2 Storage-3EA |
| ERS | Source4 1530 | HPL750W | 15˚~30˚ | 13.2kg | 47 | ETC | Front Side SL-18EA  Front Side SR-18EA  #2 Storage-11EA |
| ERS | Source4 2550 | HPL750W | 25˚~50˚ | 12.7kg | 14 | ETC | #2 Storage-14EA |
| ERS | Source4 26 | HPL750W | 26˚ | 9.1kg | 22 | ETC | #2 Storage-22EA |
| ERS | Source4 36 | HPL750W | 36˚ | 9.1kg | 28 | ETC | Side Stand-16EA  #2 Storage-12EA |
| ERS | Source4 50 | HPL750W | 50˚ | 9.1kg | 11 | ETC | #2 Storage-11EA |
| **Item** | **Model** | **Lamp type** | **Angle** | **Weight** | **Quantity** | **Origin** | **Remarks** |
| PAR | PAR 64 | CP 61 1kW | 13˚ |  | 42 | Korea | #2 Storage-42EA |
| PAR | PAR 64 | CP 62 1kW | 23˚~25˚ |  | 104 | Korea | #2 Storage-104EA |
| PAR | PAR 46 | 28V 250W |  |  | 92 | Korea | #2 Storage  black-68EA  silver-24EA |

**Fog**

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Item** | **Model** | **Weight** | **Power Consumption** | **Quantity** | **Origin** | **Remarks** |
| Haze | Unique 2 | 8.7kg | 1500W | 2 | Look solutions | #2 Storage |
| Fog | Viper 2.6 | 12kg | 2600W | 2 | Look solutions | #2 Storage |
| Fazer | Z-380 | 8.3kg | 1500W | 2 | Antari | #2 Storage |
| Fan |  |  |  | 2 | China | #2 Storage |
| Low Fog | DNG-200 | 120kg | 2500W | 4 | Antari | PIT Storage |

**Accessory**

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Item** | **Model** | **type** | **Weight** | **Quantity** | **Origin** | **Remarks** |
| Iris | Source4 |  |  | 27 | ETC | #3 Storage |
| Iris | DN205 |  |  | 30 | ADB | Ceiling Cabinet |
| Gobo Holder | Source4 |  |  | 123 | ETC | #3 Storage |
| Gobo Holder | DN205 |  |  | 30 | ADB | Ceiling Cabinet |
| Top Hat | Quantum Wash |  |  | 20 | Korea | #3 Storage |
| Top Hat | Source4 Standard |  |  | 17 |  | #3 Storage |
| Top Hat | Source4 Zoom |  |  | 13 |  | #1 Storage |
| Barn door | 5kW Marumo |  |  | 3 | Marumo | #2 Storage |
| Stand | Boom Stand | 4m |  | 2 | Korea | #2 Storage |
| Stand | Boom Stand | 2m |  | 4 | Korea | #2 Storage |
| Stand | Side Stand 2단(silver) | 1.5m |  | 8 | Korea | #2 Storage |
| Stand | SHB-10 Foot Stand | 0.05m |  | 6 | Marumo | #3 Storage |